


Header Info string subVi not implemented in older instrument classes including tool



DataNames update not possible once display name initialized



Solution : Force erase the DatDisplay names that need to be updated into Header Action:



11 fev 2021 Adding single point tables acquisition type to data

The idea here is to replicate the start acq case into to main q to be call by array instrument type like camera, i.e.: instrument that produce a complete curve or multiple curve in one acquisition. Like spectrographic cam or VNA’s, spectrum anylizer

